Peripheral Memory Device

Supports PEN and PENCIL inputs concurrently.

Encodes output to 2-Demintional photon-deflection matric in real time at a bit rate bound only by the speed of light.

Supports all open-source visual communication protocol such as English, Spanish, Arabic Numerals, Roman Numerals, sketch, etc. as well as user-defined protocols.

Multi-thread access to individual pages with automatically managed read-write permissions.

Storage stable for up to 1000 years when stored properly.

Capacity: 816 KB